**Interactive Projector**

* Should support Two additional display
* WXGA , 3500 ANSILUMENS
* Contrast ration 14000:1
* 16 watts speakers
* Screen Size (Projected Distance): 60” - 100” [35.4 - 60.1 cm] 74.3” screen 44.3cm
* Interactive Pen Digital Pen (Easy Interactive Pen 1,2)
* Fingers: Finger (1-6 fingers)
* Calibration Method: Pen: Auto / Manual (25points)
* Finger: Manual (16points)
* Vertical/Horizontal: ±3° / ±3°Quick Corner: Yes
* Network: Wired LAN RJ45 x 1 (100Mbps)
* Analog Input: D-Sub 15Pin: 2 (Blue)
* Composite: RCA x 1 (Yellow)Digital Input: HDMI: 3 (HDMI1 in common with MHL)
* Output Terminal: D-Sub 15Pin:1 (Black) In common with Computer2
* Audio Input: Stereo Mini Jack: 3
* Audio Output: Stereo Mini Jack: 1
* Control I/O: RS-232C: D-Sub 9pin x 1
* Interactive Sync: Stereo Mini Jack IN x 1, OUT x 1
* Others: USB Type A: 1 (for USB Memory, USB Document Camera, Firmware
* Update, Copy OSD Settings)
* USB Type B: 1 (for USB Display, Mouse, K/B, Control, Firmware Update, Interactive,
* Copy OSD Settings)
* Warranty – Lamp – 1000 hours , Product – 2years
* Support the facility to Split the projector screen into two to project images from two different sources simultaneously.
* Support the facility to project from presenter’s laptop wirelessly using software to up to 50 laptops and mobile devices
* Facility to send a projected image with questions to all connected participant devices.
* Facility to view thumbnail previews of the answers on participant’s devices and select up to four of them to be projected on the screen simultaneously for sharing and comparison.